From fc8e9c54699e42754094ff475da46440778d8f19 Mon Sep 17 00:00:00 2001
From: Junwei Zhang <Jerry.Zhang@amd.com>
Date: Thu, 4 Aug 2016 12:54:22 +0800
Subject: [PATCH] drm/amd/amdgpu: add Polaris12 PCI ID
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Junwei Zhang <Jerry.Zhang@amd.com>
Reviewed-by: Alex Deucher <alexander.deucher@amd.com>
Reviewed-by: Christian König <christian.koenig@amd.com>
Reviewed-by: Ken Wang  <Qingqing.Wang@amd.com>
Signed-off-by: Alex Deucher <alexander.deucher@amd.com>
---
 drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c b/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c
index 8cb937b..2534ada 100644
--- a/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c
+++ b/drivers/gpu/drm/amd/amdgpu/amdgpu_drv.c
@@ -418,6 +418,13 @@ static const struct pci_device_id pciidlist[] = {
 	{0x1002, 0x67CA, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS10},
 	{0x1002, 0x67CC, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS10},
 	{0x1002, 0x67CF, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS10},
+	/* Polaris12 */
+	{0x1002, 0x6980, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS12},
+	{0x1002, 0x6981, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS12},
+	{0x1002, 0x6985, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS12},
+	{0x1002, 0x6986, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS12},
+	{0x1002, 0x6987, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS12},
+	{0x1002, 0x699F, PCI_ANY_ID, PCI_ANY_ID, 0, 0, CHIP_POLARIS12},
 
 	{0, 0, 0}
 };
-- 
2.10.2

